**RL v2.26.0 API Release Notes:**

**New Endpoints:**

|  |  |  |
| --- | --- | --- |
| POST | /devices/{device\_id}/install\_report | Manually add an install report to a device without one. |
| GET | /installerapp/devices/{device\_sn} | Get installation report by device IMEI |

**Updated Endpoints:**

|  |  |  |
| --- | --- | --- |
| PUT | /companies/{company\_name} | live\_active, trace\_active, and storage\_active are no longer required form-data fields.Default values changed to the following:* trace\_active = true
* storage\_active = true
* billing\_date = 1

For backwards compatibility, these form-data values can still be passed **but we highly encourage developers to no longer pass these values into the request**. In the future we reserve the right to no longer accept these form-data values. |
| POST | /companies/{company\_name} | live\_active, trace\_active, and storage\_active are no longer required form-data fields.For backwards compatibility, these form-data values can still be passed **but we highly encourage developers to no longer pass these values into the request**. In the future we reserve the right to no longer accept these form-data values. |
| GET | /profiles/{profile\_id} | Added “Seatbelt” event object to “Dms” object. |
| POST | /users/updatenotifications/{email} | New parameter:* “alert\_camera\_failure” (Channel Status notification)

Removed parameter:* vehicle\_email
 |
| GET | /users/updatenotifications/{email} | New parameter in response object:email: boolean |
| POST | /partners/companies/{company\_name}/profiles | Added the following form-data fields where possible valid values are one of “alert\_only”, “snapshot\_only”, or “video\_snapshot”* dv4\_driver
* dv4\_ext\_driver
* dv4\_high\_speed
* dv4\_fatal\_gsensor
* dv4\_distraction
* dv4\_drowsiness
* dv4\_phone\_use
* dv6\_driver
* dv6\_high\_speed
* dv6\_fatal\_gsensor
* dv6\_distraction
* dv6\_drowsiness
* dv6\_phone\_use
* dv6\_yawning
* dv6\_harsh\_braking
* dv6\_harsh\_accel
* dv6\_forward\_collision
* dv6\_headway\_monitoring
* dv6\_following\_distance
 |

**Updated Objects:**

*Device Object*

**Added**

|  |  |  |
| --- | --- | --- |
| ***key*** | ***type*** | ***description*** |
| data\_online | boolean | If true, device is sending GPS data to server |

*Relevant APIs*

* *PUT* /partners/companies/{company\_name}/devices
* *GET, POST* partners/devices/{device\_id}
* *GET* /partners/devices/search
* *GET* /partners/companies/{company\_name/groups/{group\_name}/devices

*User Notification Object*

**Added**

|  |  |  |
| --- | --- | --- |
| ***key*** | ***type*** | ***description*** |
| email | boolean | If true, user will receive this notification in their email |

*Relevant APIs*

* *GET* /users/updatenotifications/{email}